|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| XML Name | Sample value | Chirp field | Sample value | Translation |
| Channel Name= | "ctcss 67.0" | Name |  |  |
| chanIndex= | "0" | Location |  |  |
| <BandWidth> | 0 | Mode |  |  |
| <TxFreq> | 400.025 |  |  |  |
| <RxFreq> | 400.025 | Frequency |  |  |
| <TxPowerLevel> | 2 | Power |  |  |
| <AnaTxCTCFlag> | 1 |  |  | 1= CTCSS 2= DCS |
| <AnaRxCTCFlag> | 1 |  |  |  |
| <AnaTxCTCIndex> | 0 |  |  | Frequency index starting at 0 |
| <AnaRxCTCIndex> | 0 |  |  |  |
| <FreqStep> | 2 |  |  |  |
| <FreqReverseFlag> | 0 |  |  |  |
| <EncryptFlag> | 0 |  |  |  |
| <BusyNoTx> | 0 |  |  |  |
| <PTTIdFlag> | 0 |  |  |  |
| <DTMFDecode> | 0 |  |  |  |
| <AMChanFlag> | 0 |  |  |  |